(module RPi_Pico_SMD_TH (layer F.Cu) (tedit 5F638C80)
  (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
  (tags "Through hole pin header THT 2x20 2.54mm double row")
  (fp_text reference REF** (at 0 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value RPi_Pico_SMD_TH (at 0 2.159) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.1 25.5) (end 1.5 25.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 25.5) (end -1.1 25.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 25.5) (end 3.7 25.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 15.1) (end 10.5 15.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 7.4) (end 10.5 7.8) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -18) (end 10.5 -17.6) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -25.5) (end 10.5 -25.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -2.7) (end 10.5 -2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 12.5) (end 10.5 12.9) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -7.8) (end 10.5 -7.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -12.9) (end 10.5 -12.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -0.2) (end 10.5 0.2) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 4.9) (end 10.5 5.3) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 20.1) (end 10.5 20.5) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 22.7) (end 10.5 23.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 17.6) (end 10.5 18) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -15.4) (end 10.5 -15) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -23.1) (end 10.5 -22.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -20.5) (end 10.5 -20.1) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 10) (end 10.5 10.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 2.3) (end 10.5 2.7) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -5.3) (end 10.5 -4.9) (layer F.SilkS) (width 0.12))
  (fp_line (start 10.5 -10.4) (end 10.5 -10) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 22.7) (end -10.5 23.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 20.1) (end -10.5 20.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 17.6) (end -10.5 18) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 15.1) (end -10.5 15.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 12.5) (end -10.5 12.9) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 10) (end -10.5 10.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 7.4) (end -10.5 7.8) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 4.9) (end -10.5 5.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 2.3) (end -10.5 2.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -0.2) (end -10.5 0.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -2.7) (end -10.5 -2.3) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -5.3) (end -10.5 -4.9) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -7.8) (end -10.5 -7.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -10.4) (end -10.5 -10) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -12.9) (end -10.5 -12.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -15.4) (end -10.5 -15) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -18) (end -10.5 -17.6) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -20.5) (end -10.5 -20.1) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -23.1) (end -10.5 -22.7) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -25.5) (end -10.5 -25.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -7.493 -22.833) (end -7.493 -25.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -22.833) (end -7.493 -22.833) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.7 25.5) (end -10.5 25.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -10.5 -25.5) (end 10.5 -25.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -11 26) (end -11 -26) (layer F.CrtYd) (width 0.12))
  (fp_line (start 11 26) (end -11 26) (layer F.CrtYd) (width 0.12))
  (fp_line (start 11 -26) (end 11 26) (layer F.CrtYd) (width 0.12))
  (fp_line (start -11 -26) (end 11 -26) (layer F.CrtYd) (width 0.12))
  (fp_line (start -10.5 -24.2) (end -9.2 -25.5) (layer F.Fab) (width 0.12))
  (fp_line (start -10.5 25.5) (end -10.5 -25.5) (layer F.Fab) (width 0.12))
  (fp_line (start 10.5 25.5) (end -10.5 25.5) (layer F.Fab) (width 0.12))
  (fp_line (start 10.5 -25.5) (end 10.5 25.5) (layer F.Fab) (width 0.12))
  (fp_line (start -10.5 -25.5) (end 10.5 -25.5) (layer F.Fab) (width 0.12))
  (fp_text user %R (at 0 0 180) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GP1 (at -12.9 -21.6 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP2 (at -12.9 -16.51 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP0 (at -12.8 -24.13 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP3 (at -12.8 -13.97 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP4 (at -12.8 -11.43 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP5 (at -12.8 -8.89 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP6 (at -12.8 -3.81 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP7 (at -12.7 -1.3 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP8 (at -12.8 1.27 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP9 (at -12.8 3.81 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP10 (at -13.054 8.89 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP11 (at -13.2 11.43 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP12 (at -13.2 13.97 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP13 (at -13.054 16.51 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP14 (at -13.1 21.59 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP15 (at -13.054 24.13 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP16 (at 13.054 24.13 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP17 (at 13.054 21.59 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP18 (at 13.054 16.51 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP19 (at 13.054 13.97 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP20 (at 13.054 11.43 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP21 (at 13.054 8.9 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP22 (at 13.054 3.81 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user RUN (at 13 1.27 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP26 (at 13.054 -1.27 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP27 (at 13.054 -3.8 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GP28 (at 13.054 -9.144 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user ADC_VREF (at 14 -12.5 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user 3V3 (at 12.9 -13.9 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user 3V3_EN (at 13.7 -17.2 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user VSYS (at 13.2 -21.59 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user VBUS (at 13.3 -24.2 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at -12.8 -19.05 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at -12.8 -6.35 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at -12.8 6.35 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at -12.8 19.05 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at 12.8 19.05 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at 12.8 6.35 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user GND (at 12.8 -19.05 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user AGND (at 13.054 -6.35 45) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user SWCLK (at -5.7 26.2) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text user SWDIO (at 5.6 26.2) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_poly (pts (xy -1.5 -16.5) (xy -3.5 -16.5) (xy -3.5 -18.5) (xy -1.5 -18.5)) (layer Dwgs.User) (width 0.1))
  (fp_poly (pts (xy -1.5 -14) (xy -3.5 -14) (xy -3.5 -16) (xy -1.5 -16)) (layer Dwgs.User) (width 0.1))
  (fp_poly (pts (xy -1.5 -11.5) (xy -3.5 -11.5) (xy -3.5 -13.5) (xy -1.5 -13.5)) (layer Dwgs.User) (width 0.1))
  (fp_poly (pts (xy 3.7 -20.2) (xy -3.7 -20.2) (xy -3.7 -24.9) (xy 3.7 -24.9)) (layer Dwgs.User) (width 0.1))
  (fp_text user "Copper Keepouts shown on Dwgs layer" (at 0.1 -30.2) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole oval (at -8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at -8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 3 thru_hole rect (at -8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at -8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at -8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at -8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at -8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 8 thru_hole rect (at -8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at -8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at -8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at -8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 12 thru_hole oval (at -8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 13 thru_hole rect (at -8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 14 thru_hole oval (at -8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 15 thru_hole oval (at -8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 16 thru_hole oval (at -8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 17 thru_hole oval (at -8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 18 thru_hole rect (at -8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 19 thru_hole oval (at -8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 20 thru_hole oval (at -8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 21 thru_hole oval (at 8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 22 thru_hole oval (at 8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 23 thru_hole rect (at 8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 24 thru_hole oval (at 8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 25 thru_hole oval (at 8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 26 thru_hole oval (at 8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 27 thru_hole oval (at 8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 28 thru_hole rect (at 8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 29 thru_hole oval (at 8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 30 thru_hole oval (at 8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 31 thru_hole oval (at 8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 32 thru_hole oval (at 8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 33 thru_hole rect (at 8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 34 thru_hole oval (at 8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 35 thru_hole oval (at 8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 36 thru_hole oval (at 8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 37 thru_hole oval (at 8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 38 thru_hole rect (at 8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 39 thru_hole oval (at 8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 40 thru_hole oval (at 8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 1 smd rect (at -8.89 -24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 2 smd rect (at -8.89 -21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 3 smd rect (at -8.89 -19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 4 smd rect (at -8.89 -16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 5 smd rect (at -8.89 -13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 6 smd rect (at -8.89 -11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 7 smd rect (at -8.89 -8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 8 smd rect (at -8.89 -6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 9 smd rect (at -8.89 -3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 10 smd rect (at -8.89 -1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 11 smd rect (at -8.89 1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 12 smd rect (at -8.89 3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 13 smd rect (at -8.89 6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 14 smd rect (at -8.89 8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 15 smd rect (at -8.89 11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 16 smd rect (at -8.89 13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 17 smd rect (at -8.89 16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 18 smd rect (at -8.89 19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 19 smd rect (at -8.89 21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 20 smd rect (at -8.89 24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 40 smd rect (at 8.89 -24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 39 smd rect (at 8.89 -21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 38 smd rect (at 8.89 -19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 37 smd rect (at 8.89 -16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 36 smd rect (at 8.89 -13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 35 smd rect (at 8.89 -11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 34 smd rect (at 8.89 -8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 33 smd rect (at 8.89 -6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 32 smd rect (at 8.89 -3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 31 smd rect (at 8.89 -1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 30 smd rect (at 8.89 1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 29 smd rect (at 8.89 3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 28 smd rect (at 8.89 6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 27 smd rect (at 8.89 8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 26 smd rect (at 8.89 11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 25 smd rect (at 8.89 13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 24 smd rect (at 8.89 16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 23 smd rect (at 8.89 19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 22 smd rect (at 8.89 21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad 21 smd rect (at 8.89 24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask))
  (pad "" np_thru_hole oval (at -2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  (pad 41 smd rect (at -2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 41 thru_hole oval (at -2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 42 smd rect (at 0 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 42 thru_hole rect (at 0 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
  (pad 43 smd rect (at 2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask))
  (pad 43 thru_hole oval (at 2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask))
)
